Thermal ID spec

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Therm | Dev | Polling | ambient\_sensor | 0x1 |
| Therm | Dev | Polling | cpu\_status\_tdev | 0x2 |
| Therm | Dev | Polling | cpu\_dts\_tdev | 0x3 |
| Therm | Dev | Polling | cpu\_power\_tdev | 0x4 |
| Therm | Dev | Polling | cpu\_vr\_tdev | 0x5 |
| Therm | Dev | Polling | cpu\_tdp | 0x6 |
| Therm | Dev | Polling | dimm\_proxy\_tdev | 0x7 |
| Therm | Dev | Polling | dimm\_tdev | 0x8 |
| Therm | Dev | Polling | drive\_temp\_tdev | 0x9 |
| Therm | Dev | Polling | dimm\_vr\_tdev | 0x10 |
| Therm | Dev | Polling | fan\_proxy | 0x11 |
| Therm | Dev | Polling | fan\_sensor | 0x12 |
| Therm | Dev | Polling | m2\_drive\_tdev | 0x13 |
| Therm | Dev | Polling | m2\_ambient\_tdev | 0x14 |
| Therm | Dev | Polling | pch\_temp\_dev | 0x15 |
| Therm | Dev | Polling | psu\_inlet\_temp | 0x16 |
| Therm | Dev | Polling | pci\_tdev | 0x17 |
| Therm | Dev | Polling | pldm\_tdev | 0x18 |
| Therm | Dev | Polling | raid\_card\_tdev | 0x19 |
| Therm | Dev | Polling | raid\_cap\_tdev | 0x20 |
| Therm | Dev | Polling | r7\_drive\_temp | 0x21 |